Disincentive Strength Concrete Pavement, Item 804.6050 – Example DT1310 (NER20-0116)

* **Bid Item Name:**

Disincentive Strength Concrete Pavement, Item 804.6050

* **Quantity Involved:**

Enter dollar amount of disincentive

* **Units:**

DOL

* **Test Results:**

See Disposition Explanation

* **Spec Requirements:**

SS 715.5.1(4)

Strength >= 3,700 psi

* **Disposition Explanation:**

Concrete pavement compressive strength was reported below minimum strength. Data was reviewed by project staff and pay was adjusted according to SS 715.5.2.

Lot/Sublot:

 6-5 (-$656.60)

Disincentives are applied in CCO #2.

* **Placement Date:**

Leave Blank

* **Sample Date:**

Leave Blank

* **Sample Location:**

See HQMS

* **Usage:**

Concrete Pavement 8-Inch

* **Usage Location:**

See Disposition Explanation



Figure: MIT Entry Disincentive Strength Concrete Pavement Example



Figure: Printed DT1310 Disincentive Strength Concrete Pavement Example