TRAFFIC CONTROL INSPECTION CHECKLIST

Project I.D:	Hwy:	County:

Date:	Road Open Road Closed To Thru Traffic	Responsible Engineer (Inspector):

Traffic Control Devices	Evaluate (A = Acceptable, M = Marginal, U =Unacceptable)	Any Missing Devices	No. of Devices	Description, Comments or Corrective measures recommended (Use reverse side, if necessary)
Condition	Placement & Spacing	Visibility Day & Night	General Effectiveness
Signs & Sign Mounting
Detour Signs
Barricades
Drums
Type A, Flashing Lights
Type C, Steady Burn Lights
Arrow Panel
Flexible Tabular Markers
Temporary Barrier
Cones
Temporary Delineators
Pavement Marking & Conflicting Marking Removal
Temp. Raised Pavement Marker
Temporary Crash Cushions
Others

Time of Inspection	Signature	Weather Conditions	Comments and/or Corrective Action
AM PM

Comments on:

Pavement Condition:

Detour:

Temporary Roads/Crossovers:

Flagger Equipment/ procedures:

Protection of manholes, dropoffs, hazards for peds, bikes, etc:

Equipment/Material storage location:

Do any previously reported discrepancies still exist?	If so, describe:

Acceptable:	Devices that meet all requirements such as design, size, color, reflectivity, etc. in the plan and specifications.
Marginal:	Devices that are marginally acceptable and they are reaching the lower end of acceptability. The color and reflectivity are still apparent at night.
Unacceptable:	Devices that do not serve the intended function, because of large abrasions or areas of residue, illegibility, lack of reflectivity, or other defects. These devices should be replaced or repaired immediately.
Distribution:	Project Files, Responsible Engineer (Inspector)

This checklist is intended primarily to assist the WisDOT inspectors, and it is NOT a contract document.