{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Instructions","Example","3-Longit. Lines","4-Longit. Lines","Locations"],"not_rendered":{"charts":0,"images":10,"macros":1,"external_links":0,"defined_names":7,"comments":3,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":92,"n_cols":5,"rows_kept":92,"cut":false,"hidden":false,"merged":[]}
["Slab Bridge Grade Computations Spreadsheet Instructions"]
[]
["Instructions:",null,null,"Assumptions:"]
["1)","There are two different tabs within the spreadsheet.  The different tabs provide ",null,"-","Project specific parameters may require additional factors to be built-in"]
[null,"options for different numbers of bridge cross-section locations that data is to be ",null,"-","Slab Thickness will vary at haunched sections near substructures.  Field engineer to modify accordingly."]
[null,"input by the field engineer.  For the 3 cross-section option, it is assumed that ",null,"-","No crushing factors have been built into this spreadsheet"]
[null,"the reference line/profile grade line/crown are all at the same location.  For the ",null,"-","3-Longitudinal Lines spreadsheet assumes a bridge cross-section per (or similar to) the image below:"]
[null,"4 cross-section option, it is assumed that the reference line/profile grade line "]
[null,"are different from the crown location.  Each of the tabs function the same way "]
[null,"aside from the number of cross-section locations to be calculated."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"-","4-Longitudinal Lines spreadsheet assumes a bridge cross-section per (or similar to) the image below:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["2)","The highlighted cells are those that need to be input by the field engineer, in "]
[null,"addition to the table values.  Within many of these cells, there are drop-down "]
[null,"boxes to select options.  The spreadsheet has been set up to accommodate up "]
[null,"to 5 spans (if a slab bridge has more than 5 spans, then additional spreadsheets "]
[null,"could be used, but this should be a rare occurrence).  Depending on the value ",null,"-","The \"Field Surveyed Top of Installed Falsework Elevation\" information is not a specific location on the"]
[null,"selected in the drop-down box for “Number of spans”, the correct number of ",null,null,"falsework.  This could be the top of steel beam, top of wood blocking on top of the steel beam, or any"]
[null,"tables below will appear for use by the field engineer.  Additionally, the ",null,null,"other location.  The \"T values\" make up the difference from the surveyed location to the bottom of the "]
[null,"spreadsheet includes drop-down menu options for the “Slab Location” areas ",null,null,"in-place slab concrete."]
[null,"being analyzed by the field engineer.  The cells that have black values auto-"]
[null,"matically shown are auto-calculated and do not need to be adjusted."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["3)","The “Top of Slab Elev”, “Slab Thickness”, and “Camber” table values should be "]
[null,"manually input by the field engineer based on the values shown in the bridge"]
[null,"plans.  The \"Falsework Settlement/Deflection\" information is to be provided to"]
[null,"the Department by the contractor.  The \"Field Surveyed Top of Installed"]
[null,"Falsework Elevation\" is also to be provided by the contractor.  Each of the"]
[null,"contractor-supplied values should be manually input by the field engineer."]
[null,"Per the standard spec, the contractor is required to provide these values at 1/10"]
[null,"point locations in order to align with the structure plan values."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["4)","The “Top of Falsework Elevation” and falsework blocking (or 'T' values) values "]
[null,"are automatically calculated based on the input values previously noted above.  "]
[null,"These values should be used in the field in order to accurately pour the slab to "]
[null,"meet the intended grades."]

{"sheet":"Example","index":1,"n_rows":94,"n_cols":13,"rows_kept":94,"cut":false,"hidden":false,"merged":[[0,0,0,12],[1,0,1,12],[2,0,2,12],[3,1,3,2],[4,1,4,2],[13,1,13,3]]}
["Slab Span Tenth Point Grades"]
["3 Cross-Section Points of Reference"]
["Wisconsin Department of Transportation"]
["Bridge Number:","B-68-133"]
["Project Construction ID:","6270-00-74"]
[null,1]
[null,2]
[null,3]
[null,4]
[null,5]
["Number of spans:",1]
[]
["Span 1"]
["Slab Location:","West Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)",null,947.48,947.46,947.45,947.44,947.42,947.41,947.39,947.38,947.36,947.35,947.33]
["- Slab Thickness (in)",null,19,19,19,19,19,19,19,19,19,19,19]
["+ Camber (in)",null,0,0.4,0.8,1.1000000000000001,1.3,1.4,1.3,1.1000000000000001,0.8,0.4,0]
["+ Falsework Settlement/Deflection (in)",null,0,0.1,0.27,0.4,0.49,0.51,0.49,0.4,0.27,0.1,0]
["= Top of Falsework Elevation",null,{"$f":"C16-(C17/12)+(C18/12)+(C19/12)","v":945.89666666666665},{"$f":"D16-(D17/12)+(D18/12)+(D19/12)","v":945.91833333333329},{"$f":"E16-(E17/12)+(E18/12)+(E19/12)","v":945.95583333333343},945.98166666666668,945.98583333333329,945.98583333333329,945.95583333333332,945.92166666666662,945.8658333333334,945.80833333333328,{"$f":"M16-(M17/12)+(M18/12)+(M19/12)","v":945.74666666666667}]
["- Field Surveyed Top of Installed Falsework Elevation",null,945.25,945.25,945.25,945.25,945.25,945.25,945.25,945.25,945.25,945.25,945.25]
["= 'T' Values (ft)",null,{"$f":"C20-C21","v":0.64666666666664696},{"$f":"D20-D21","v":0.66833333333329392},0.70583333333343035,0.73166666666668334,0.73583333333328937,0.73583333333328937,0.70583333333331666,0.67166666666662422,0.61583333333339851,0.55833333333328028,0.4966666666666697]
["= 'T' Values (in)",null,{"$f":"C22*12","v":7.7599999999997635},{"$f":"D22*12","v":8.0199999999995271},8.4700000000011642,8.7800000000002001,8.8299999999994725,8.8299999999994725,8.4699999999997999,8.0599999999994907,7.3900000000007822,6.6999999999993634,5.9600000000000364]
[]
[]
[]
[]
[]
["Top of Slab Elevations (per the Bridge plans):"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Slab Thickness (per the Bridge plans):"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Camber (per the Bridge plans):"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Falsework Deflection (per contractor's falsework plans):"]

{"sheet":"3-Longit. Lines","index":2,"n_rows":181,"n_cols":13,"rows_kept":181,"cut":false,"hidden":false,"merged":[[115,1,115,3],[3,1,3,2],[4,1,4,2],[160,1,160,3],[171,1,171,3],[35,1,35,3],[47,1,47,3],[58,1,58,3],[69,1,69,3],[81,1,81,3],[92,1,92,3],[103,1,103,3],[126,1,126,3],[137,1,137,3],[149,1,149,3],[0,0,0,12],[1,0,1,12],[2,0,2,12],[13,1,13,3],[24,1,24,3]]}
["Slab Span Tenth Point Grades"]
["3 Cross-Section Points of Reference"]
["Wisconsin Department of Transportation"]
["Bridge Number:","B-XX-XXXX"]
["Project Construction ID:","XXXX-XX-XX"]
[null,1]
[null,2]
[null,3]
[null,4]
[null,5]
["Number of spans:",5]
[]
["Span 1"]
["Slab Location:","North Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C16-(C17/12)+(C18/12)+(C19/12)","v":0},{"$f":"D16-(D17/12)+(D18/12)+(D19/12)","v":0},0,0,0,0,0,0,0,0,0]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C20-C21","v":0},{"$f":"D20-D21","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C22*12","v":0},{"$f":"D22*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Reference Line"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C27-(C28/12)+(C29/12)+(C30/12)","v":0},{"$f":"D27-(D28/12)+(D29/12)+(D30/12)","v":0},{"$f":"E27-(E28/12)+(E29/12)+(E30/12)","v":0},{"$f":"F27-(F28/12)+(F29/12)+(F30/12)","v":0},{"$f":"G27-(G28/12)+(G29/12)+(G30/12)","v":0},{"$f":"H27-(H28/12)+(H29/12)+(H30/12)","v":0},{"$f":"I27-(I28/12)+(I29/12)+(I30/12)","v":0},{"$f":"J27-(J28/12)+(J29/12)+(J30/12)","v":0},{"$f":"K27-(K28/12)+(K29/12)+(K30/12)","v":0},{"$f":"L27-(L28/12)+(L29/12)+(L30/12)","v":0},{"$f":"M27-(M28/12)+(M29/12)+(M30/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C31-C32","v":0},{"$f":"D31-D32","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C33*12","v":0},{"$f":"D33*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","South Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C38-(C39/12)+(C40/12)+(C41/12)","v":0},{"$f":"D38-(D39/12)+(D40/12)+(D41/12)","v":0},{"$f":"E38-(E39/12)+(E40/12)+(E41/12)","v":0},{"$f":"F38-(F39/12)+(F40/12)+(F41/12)","v":0},{"$f":"G38-(G39/12)+(G40/12)+(G41/12)","v":0},{"$f":"H38-(H39/12)+(H40/12)+(H41/12)","v":0},{"$f":"I38-(I39/12)+(I40/12)+(I41/12)","v":0},{"$f":"J38-(J39/12)+(J40/12)+(J41/12)","v":0},{"$f":"K38-(K39/12)+(K40/12)+(K41/12)","v":0},{"$f":"L38-(L39/12)+(L40/12)+(L41/12)","v":0},{"$f":"M38-(M39/12)+(M40/12)+(M41/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C42-C43","v":0},{"$f":"D42-D43","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C44*12","v":0},{"$f":"D44*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Span 2"]
["Slab Location:","North Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C50-(C51/12)+(C52/12)+(C53/12)","v":0},{"$f":"D50-(D51/12)+(D52/12)+(D53/12)","v":0},{"$f":"E50-(E51/12)+(E52/12)+(E53/12)","v":0},{"$f":"F50-(F51/12)+(F52/12)+(F53/12)","v":0},{"$f":"G50-(G51/12)+(G52/12)+(G53/12)","v":0},{"$f":"H50-(H51/12)+(H52/12)+(H53/12)","v":0},{"$f":"I50-(I51/12)+(I52/12)+(I53/12)","v":0},{"$f":"J50-(J51/12)+(J52/12)+(J53/12)","v":0},{"$f":"K50-(K51/12)+(K52/12)+(K53/12)","v":0},{"$f":"L50-(L51/12)+(L52/12)+(L53/12)","v":0},{"$f":"M50-(M51/12)+(M52/12)+(M53/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C54-C55","v":0},{"$f":"D54-D55","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C56*12","v":0},{"$f":"D56*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Reference Line"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C61-(C62/12)+(C63/12)+(C64/12)","v":0},{"$f":"D61-(D62/12)+(D63/12)+(D64/12)","v":0},{"$f":"E61-(E62/12)+(E63/12)+(E64/12)","v":0},{"$f":"F61-(F62/12)+(F63/12)+(F64/12)","v":0},{"$f":"G61-(G62/12)+(G63/12)+(G64/12)","v":0},{"$f":"H61-(H62/12)+(H63/12)+(H64/12)","v":0},{"$f":"I61-(I62/12)+(I63/12)+(I64/12)","v":0},{"$f":"J61-(J62/12)+(J63/12)+(J64/12)","v":0},{"$f":"K61-(K62/12)+(K63/12)+(K64/12)","v":0},{"$f":"L61-(L62/12)+(L63/12)+(L64/12)","v":0},{"$f":"M61-(M62/12)+(M63/12)+(M64/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C65-C66","v":0},{"$f":"D65-D66","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C67*12","v":0},{"$f":"D67*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","South Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C72-(C73/12)+(C74/12)+(C75/12)","v":0},{"$f":"D72-(D73/12)+(D74/12)+(D75/12)","v":0},{"$f":"E72-(E73/12)+(E74/12)+(E75/12)","v":0},{"$f":"F72-(F73/12)+(F74/12)+(F75/12)","v":0},{"$f":"G72-(G73/12)+(G74/12)+(G75/12)","v":0},{"$f":"H72-(H73/12)+(H74/12)+(H75/12)","v":0},{"$f":"I72-(I73/12)+(I74/12)+(I75/12)","v":0},{"$f":"J72-(J73/12)+(J74/12)+(J75/12)","v":0},{"$f":"K72-(K73/12)+(K74/12)+(K75/12)","v":0},{"$f":"L72-(L73/12)+(L74/12)+(L75/12)","v":0},{"$f":"M72-(M73/12)+(M74/12)+(M75/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C76-C77","v":0},{"$f":"D76-D77","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C78*12","v":0},{"$f":"D78*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Span 3"]
["Slab Location:","North Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C84-(C85/12)+(C86/12)+(C87/12)","v":0},{"$f":"D84-(D85/12)+(D86/12)+(D87/12)","v":0},{"$f":"E84-(E85/12)+(E86/12)+(E87/12)","v":0},{"$f":"F84-(F85/12)+(F86/12)+(F87/12)","v":0},{"$f":"G84-(G85/12)+(G86/12)+(G87/12)","v":0},{"$f":"H84-(H85/12)+(H86/12)+(H87/12)","v":0},{"$f":"I84-(I85/12)+(I86/12)+(I87/12)","v":0},{"$f":"J84-(J85/12)+(J86/12)+(J87/12)","v":0},{"$f":"K84-(K85/12)+(K86/12)+(K87/12)","v":0},{"$f":"L84-(L85/12)+(L86/12)+(L87/12)","v":0},{"$f":"M84-(M85/12)+(M86/12)+(M87/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C88-C89","v":0},{"$f":"D88-D89","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C90*12","v":0},{"$f":"D90*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Reference Line"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C95-(C96/12)+(C97/12)+(C98/12)","v":0},{"$f":"D95-(D96/12)+(D97/12)+(D98/12)","v":0},{"$f":"E95-(E96/12)+(E97/12)+(E98/12)","v":0},{"$f":"F95-(F96/12)+(F97/12)+(F98/12)","v":0},{"$f":"G95-(G96/12)+(G97/12)+(G98/12)","v":0},{"$f":"H95-(H96/12)+(H97/12)+(H98/12)","v":0},{"$f":"I95-(I96/12)+(I97/12)+(I98/12)","v":0},{"$f":"J95-(J96/12)+(J97/12)+(J98/12)","v":0},{"$f":"K95-(K96/12)+(K97/12)+(K98/12)","v":0},{"$f":"L95-(L96/12)+(L97/12)+(L98/12)","v":0},{"$f":"M95-(M96/12)+(M97/12)+(M98/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C99-C100","v":0},{"$f":"D99-D100","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C101*12","v":0},{"$f":"D101*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","South Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C106-(C107/12)+(C108/12)+(C109/12)","v":0},{"$f":"D106-(D107/12)+(D108/12)+(D109/12)","v":0},{"$f":"E106-(E107/12)+(E108/12)+(E109/12)","v":0},{"$f":"F106-(F107/12)+(F108/12)+(F109/12)","v":0},{"$f":"G106-(G107/12)+(G108/12)+(G109/12)","v":0},{"$f":"H106-(H107/12)+(H108/12)+(H109/12)","v":0},{"$f":"I106-(I107/12)+(I108/12)+(I109/12)","v":0},{"$f":"J106-(J107/12)+(J108/12)+(J109/12)","v":0},{"$f":"K106-(K107/12)+(K108/12)+(K109/12)","v":0},{"$f":"L106-(L107/12)+(L108/12)+(L109/12)","v":0},{"$f":"M106-(M107/12)+(M108/12)+(M109/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C110-C111","v":0},{"$f":"D110-D111","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C112*12","v":0},{"$f":"D112*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Span 4"]
["Slab Location:","North Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C118-(C119/12)+(C120/12)+(C121/12)","v":0},{"$f":"D118-(D119/12)+(D120/12)+(D121/12)","v":0},{"$f":"E118-(E119/12)+(E120/12)+(E121/12)","v":0},{"$f":"F118-(F119/12)+(F120/12)+(F121/12)","v":0},{"$f":"G118-(G119/12)+(G120/12)+(G121/12)","v":0},{"$f":"H118-(H119/12)+(H120/12)+(H121/12)","v":0},{"$f":"I118-(I119/12)+(I120/12)+(I121/12)","v":0},{"$f":"J118-(J119/12)+(J120/12)+(J121/12)","v":0},{"$f":"K118-(K119/12)+(K120/12)+(K121/12)","v":0},{"$f":"L118-(L119/12)+(L120/12)+(L121/12)","v":0},{"$f":"M118-(M119/12)+(M120/12)+(M121/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C122-C123","v":0},{"$f":"D122-D123","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C124*12","v":0},{"$f":"D124*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Reference Line"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C129-(C130/12)+(C131/12)+(C132/12)","v":0},{"$f":"D129-(D130/12)+(D131/12)+(D132/12)","v":0},{"$f":"E129-(E130/12)+(E131/12)+(E132/12)","v":0},{"$f":"F129-(F130/12)+(F131/12)+(F132/12)","v":0},{"$f":"G129-(G130/12)+(G131/12)+(G132/12)","v":0},{"$f":"H129-(H130/12)+(H131/12)+(H132/12)","v":0},{"$f":"I129-(I130/12)+(I131/12)+(I132/12)","v":0},{"$f":"J129-(J130/12)+(J131/12)+(J132/12)","v":0},{"$f":"K129-(K130/12)+(K131/12)+(K132/12)","v":0},{"$f":"L129-(L130/12)+(L131/12)+(L132/12)","v":0},{"$f":"M129-(M130/12)+(M131/12)+(M132/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C133-C134","v":0},{"$f":"D133-D134","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C135*12","v":0},{"$f":"D135*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","South Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C140-(C141/12)+(C142/12)+(C143/12)","v":0},{"$f":"D140-(D141/12)+(D142/12)+(D143/12)","v":0},{"$f":"E140-(E141/12)+(E142/12)+(E143/12)","v":0},{"$f":"F140-(F141/12)+(F142/12)+(F143/12)","v":0},{"$f":"G140-(G141/12)+(G142/12)+(G143/12)","v":0},{"$f":"H140-(H141/12)+(H142/12)+(H143/12)","v":0},{"$f":"I140-(I141/12)+(I142/12)+(I143/12)","v":0},{"$f":"J140-(J141/12)+(J142/12)+(J143/12)","v":0},{"$f":"K140-(K141/12)+(K142/12)+(K143/12)","v":0},{"$f":"L140-(L141/12)+(L142/12)+(L143/12)","v":0},{"$f":"M140-(M141/12)+(M142/12)+(M143/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C144-C145","v":0},{"$f":"D144-D145","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C146*12","v":0},{"$f":"D146*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Span 5"]
["Slab Location:","North Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C152-(C153/12)+(C154/12)+(C155/12)","v":0},{"$f":"D152-(D153/12)+(D154/12)+(D155/12)","v":0},{"$f":"E152-(E153/12)+(E154/12)+(E155/12)","v":0},{"$f":"F152-(F153/12)+(F154/12)+(F155/12)","v":0},{"$f":"G152-(G153/12)+(G154/12)+(G155/12)","v":0},{"$f":"H152-(H153/12)+(H154/12)+(H155/12)","v":0},{"$f":"I152-(I153/12)+(I154/12)+(I155/12)","v":0},{"$f":"J152-(J153/12)+(J154/12)+(J155/12)","v":0},{"$f":"K152-(K153/12)+(K154/12)+(K155/12)","v":0},{"$f":"L152-(L153/12)+(L154/12)+(L155/12)","v":0},{"$f":"M152-(M153/12)+(M154/12)+(M155/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C156-C157","v":0},{"$f":"D156-D157","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C158*12","v":0},{"$f":"D158*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Reference Line"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C163-(C164/12)+(C165/12)+(C166/12)","v":0},{"$f":"D163-(D164/12)+(D165/12)+(D166/12)","v":0},{"$f":"E163-(E164/12)+(E165/12)+(E166/12)","v":0},{"$f":"F163-(F164/12)+(F165/12)+(F166/12)","v":0},{"$f":"G163-(G164/12)+(G165/12)+(G166/12)","v":0},{"$f":"H163-(H164/12)+(H165/12)+(H166/12)","v":0},{"$f":"I163-(I164/12)+(I165/12)+(I166/12)","v":0},{"$f":"J163-(J164/12)+(J165/12)+(J166/12)","v":0},{"$f":"K163-(K164/12)+(K165/12)+(K166/12)","v":0},{"$f":"L163-(L164/12)+(L165/12)+(L166/12)","v":0},{"$f":"M163-(M164/12)+(M165/12)+(M166/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C167-C168","v":0},{"$f":"D167-D168","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C169*12","v":0},{"$f":"D169*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","South Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C174-(C175/12)+(C176/12)+(C177/12)","v":0},{"$f":"D174-(D175/12)+(D176/12)+(D177/12)","v":0},{"$f":"E174-(E175/12)+(E176/12)+(E177/12)","v":0},{"$f":"F174-(F175/12)+(F176/12)+(F177/12)","v":0},{"$f":"G174-(G175/12)+(G176/12)+(G177/12)","v":0},{"$f":"H174-(H175/12)+(H176/12)+(H177/12)","v":0},{"$f":"I174-(I175/12)+(I176/12)+(I177/12)","v":0},{"$f":"J174-(J175/12)+(J176/12)+(J177/12)","v":0},{"$f":"K174-(K175/12)+(K176/12)+(K177/12)","v":0},{"$f":"L174-(L175/12)+(L176/12)+(L177/12)","v":0},{"$f":"M174-(M175/12)+(M176/12)+(M177/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C178-C179","v":0},{"$f":"D178-D179","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C180*12","v":0},{"$f":"D180*12","v":0},0,0,0,0,0,0,0,0,0]

{"sheet":"4-Longit. Lines","index":3,"n_rows":236,"n_cols":13,"rows_kept":236,"cut":false,"hidden":false,"merged":[[24,1,24,3],[35,1,35,3],[46,1,46,3],[193,1,193,3],[3,1,3,2],[4,1,4,2],[13,1,13,3],[58,1,58,3],[69,1,69,3],[204,1,204,3],[215,1,215,3],[226,1,226,3],[0,0,0,12],[1,0,1,12],[2,0,2,12],[159,1,159,3],[170,1,170,3],[181,1,181,3],[125,1,125,3],[136,1,136,3],[148,1,148,3],[91,1,91,3],[114,1,114,3],[103,1,103,3],[80,1,80,3]]}
["Slab Span Tenth Point Grades"]
["4 Cross-Section Points of Reference"]
["Wisconsin Department of Transportation"]
["Bridge Number:","B-XX-XXXX"]
["Project Construction ID:","XXXX-XX-XX"]
[null,1]
[null,2]
[null,3]
[null,4]
[null,5]
["Number of spans:",5]
[]
["Span 1"]
["Slab Location:","East Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C16-(C17/12)+(C18/12)+(C19/12)","v":0},{"$f":"D16-(D17/12)+(D18/12)+(D19/12)","v":0},0,0,0,0,0,0,0,0,0]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C20-C21","v":0},{"$f":"D20-D21","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C22*12","v":0},{"$f":"D22*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Reference Line"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C27-(C28/12)+(C29/12)+(C30/12)","v":0},{"$f":"D27-(D28/12)+(D29/12)+(D30/12)","v":0},{"$f":"E27-(E28/12)+(E29/12)+(E30/12)","v":0},{"$f":"F27-(F28/12)+(F29/12)+(F30/12)","v":0},{"$f":"G27-(G28/12)+(G29/12)+(G30/12)","v":0},{"$f":"H27-(H28/12)+(H29/12)+(H30/12)","v":0},{"$f":"I27-(I28/12)+(I29/12)+(I30/12)","v":0},{"$f":"J27-(J28/12)+(J29/12)+(J30/12)","v":0},{"$f":"K27-(K28/12)+(K29/12)+(K30/12)","v":0},{"$f":"L27-(L28/12)+(L29/12)+(L30/12)","v":0},{"$f":"M27-(M28/12)+(M29/12)+(M30/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C31-C32","v":0},{"$f":"D31-D32","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C33*12","v":0},{"$f":"D33*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Crown"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C38-(C39/12)+(C40/12)+(C41/12)","v":0},{"$f":"D38-(D39/12)+(D40/12)+(D41/12)","v":0},{"$f":"E38-(E39/12)+(E40/12)+(E41/12)","v":0},{"$f":"F38-(F39/12)+(F40/12)+(F41/12)","v":0},{"$f":"G38-(G39/12)+(G40/12)+(G41/12)","v":0},{"$f":"H38-(H39/12)+(H40/12)+(H41/12)","v":0},{"$f":"I38-(I39/12)+(I40/12)+(I41/12)","v":0},{"$f":"J38-(J39/12)+(J40/12)+(J41/12)","v":0},{"$f":"K38-(K39/12)+(K40/12)+(K41/12)","v":0},{"$f":"L38-(L39/12)+(L40/12)+(L41/12)","v":0},{"$f":"M38-(M39/12)+(M40/12)+(M41/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C42-C43","v":0},{"$f":"D42-D43","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C44*12","v":0},{"$f":"D44*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","West Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C49-(C50/12)+(C51/12)+(C52/12)","v":0},{"$f":"D49-(D50/12)+(D51/12)+(D52/12)","v":0},{"$f":"E49-(E50/12)+(E51/12)+(E52/12)","v":0},{"$f":"F49-(F50/12)+(F51/12)+(F52/12)","v":0},{"$f":"G49-(G50/12)+(G51/12)+(G52/12)","v":0},{"$f":"H49-(H50/12)+(H51/12)+(H52/12)","v":0},{"$f":"I49-(I50/12)+(I51/12)+(I52/12)","v":0},{"$f":"J49-(J50/12)+(J51/12)+(J52/12)","v":0},{"$f":"K49-(K50/12)+(K51/12)+(K52/12)","v":0},{"$f":"L49-(L50/12)+(L51/12)+(L52/12)","v":0},{"$f":"M49-(M50/12)+(M51/12)+(M52/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C53-C54","v":0},{"$f":"D53-D54","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C55*12","v":0},{"$f":"D55*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Span 2"]
["Slab Location:","East Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C61-(C62/12)+(C63/12)+(C64/12)","v":0},{"$f":"D61-(D62/12)+(D63/12)+(D64/12)","v":0},{"$f":"E61-(E62/12)+(E63/12)+(E64/12)","v":0},{"$f":"F61-(F62/12)+(F63/12)+(F64/12)","v":0},{"$f":"G61-(G62/12)+(G63/12)+(G64/12)","v":0},{"$f":"H61-(H62/12)+(H63/12)+(H64/12)","v":0},{"$f":"I61-(I62/12)+(I63/12)+(I64/12)","v":0},{"$f":"J61-(J62/12)+(J63/12)+(J64/12)","v":0},{"$f":"K61-(K62/12)+(K63/12)+(K64/12)","v":0},{"$f":"L61-(L62/12)+(L63/12)+(L64/12)","v":0},{"$f":"M61-(M62/12)+(M63/12)+(M64/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C65-C66","v":0},{"$f":"D65-D66","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C67*12","v":0},{"$f":"D67*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Reference Line"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C72-(C73/12)+(C74/12)+(C75/12)","v":0},{"$f":"D72-(D73/12)+(D74/12)+(D75/12)","v":0},{"$f":"E72-(E73/12)+(E74/12)+(E75/12)","v":0},{"$f":"F72-(F73/12)+(F74/12)+(F75/12)","v":0},{"$f":"G72-(G73/12)+(G74/12)+(G75/12)","v":0},{"$f":"H72-(H73/12)+(H74/12)+(H75/12)","v":0},{"$f":"I72-(I73/12)+(I74/12)+(I75/12)","v":0},{"$f":"J72-(J73/12)+(J74/12)+(J75/12)","v":0},{"$f":"K72-(K73/12)+(K74/12)+(K75/12)","v":0},{"$f":"L72-(L73/12)+(L74/12)+(L75/12)","v":0},{"$f":"M72-(M73/12)+(M74/12)+(M75/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C76-C77","v":0},{"$f":"D76-D77","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C78*12","v":0},{"$f":"D78*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Crown"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C83-(C84/12)+(C85/12)+(C86/12)","v":0},{"$f":"D83-(D84/12)+(D85/12)+(D86/12)","v":0},{"$f":"E83-(E84/12)+(E85/12)+(E86/12)","v":0},{"$f":"F83-(F84/12)+(F85/12)+(F86/12)","v":0},{"$f":"G83-(G84/12)+(G85/12)+(G86/12)","v":0},{"$f":"H83-(H84/12)+(H85/12)+(H86/12)","v":0},{"$f":"I83-(I84/12)+(I85/12)+(I86/12)","v":0},{"$f":"J83-(J84/12)+(J85/12)+(J86/12)","v":0},{"$f":"K83-(K84/12)+(K85/12)+(K86/12)","v":0},{"$f":"L83-(L84/12)+(L85/12)+(L86/12)","v":0},{"$f":"M83-(M84/12)+(M85/12)+(M86/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C87-C88","v":0},{"$f":"D87-D88","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C89*12","v":0},{"$f":"D89*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","West Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C94-(C95/12)+(C96/12)+(C97/12)","v":0},{"$f":"D94-(D95/12)+(D96/12)+(D97/12)","v":0},{"$f":"E94-(E95/12)+(E96/12)+(E97/12)","v":0},{"$f":"F94-(F95/12)+(F96/12)+(F97/12)","v":0},{"$f":"G94-(G95/12)+(G96/12)+(G97/12)","v":0},{"$f":"H94-(H95/12)+(H96/12)+(H97/12)","v":0},{"$f":"I94-(I95/12)+(I96/12)+(I97/12)","v":0},{"$f":"J94-(J95/12)+(J96/12)+(J97/12)","v":0},{"$f":"K94-(K95/12)+(K96/12)+(K97/12)","v":0},{"$f":"L94-(L95/12)+(L96/12)+(L97/12)","v":0},{"$f":"M94-(M95/12)+(M96/12)+(M97/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C98-C99","v":0},{"$f":"D98-D99","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C100*12","v":0},{"$f":"D100*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Span 3"]
["Slab Location:","East Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C106-(C107/12)+(C108/12)+(C109/12)","v":0},{"$f":"D106-(D107/12)+(D108/12)+(D109/12)","v":0},{"$f":"E106-(E107/12)+(E108/12)+(E109/12)","v":0},{"$f":"F106-(F107/12)+(F108/12)+(F109/12)","v":0},{"$f":"G106-(G107/12)+(G108/12)+(G109/12)","v":0},{"$f":"H106-(H107/12)+(H108/12)+(H109/12)","v":0},{"$f":"I106-(I107/12)+(I108/12)+(I109/12)","v":0},{"$f":"J106-(J107/12)+(J108/12)+(J109/12)","v":0},{"$f":"K106-(K107/12)+(K108/12)+(K109/12)","v":0},{"$f":"L106-(L107/12)+(L108/12)+(L109/12)","v":0},{"$f":"M106-(M107/12)+(M108/12)+(M109/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C110-C111","v":0},{"$f":"D110-D111","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C112*12","v":0},{"$f":"D112*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Reference Line"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C117-(C118/12)+(C119/12)+(C120/12)","v":0},{"$f":"D117-(D118/12)+(D119/12)+(D120/12)","v":0},{"$f":"E117-(E118/12)+(E119/12)+(E120/12)","v":0},{"$f":"F117-(F118/12)+(F119/12)+(F120/12)","v":0},{"$f":"G117-(G118/12)+(G119/12)+(G120/12)","v":0},{"$f":"H117-(H118/12)+(H119/12)+(H120/12)","v":0},{"$f":"I117-(I118/12)+(I119/12)+(I120/12)","v":0},{"$f":"J117-(J118/12)+(J119/12)+(J120/12)","v":0},{"$f":"K117-(K118/12)+(K119/12)+(K120/12)","v":0},{"$f":"L117-(L118/12)+(L119/12)+(L120/12)","v":0},{"$f":"M117-(M118/12)+(M119/12)+(M120/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C121-C122","v":0},{"$f":"D121-D122","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C123*12","v":0},{"$f":"D123*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Crown"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C128-(C129/12)+(C130/12)+(C131/12)","v":0},{"$f":"D128-(D129/12)+(D130/12)+(D131/12)","v":0},{"$f":"E128-(E129/12)+(E130/12)+(E131/12)","v":0},{"$f":"F128-(F129/12)+(F130/12)+(F131/12)","v":0},{"$f":"G128-(G129/12)+(G130/12)+(G131/12)","v":0},{"$f":"H128-(H129/12)+(H130/12)+(H131/12)","v":0},{"$f":"I128-(I129/12)+(I130/12)+(I131/12)","v":0},{"$f":"J128-(J129/12)+(J130/12)+(J131/12)","v":0},{"$f":"K128-(K129/12)+(K130/12)+(K131/12)","v":0},{"$f":"L128-(L129/12)+(L130/12)+(L131/12)","v":0},{"$f":"M128-(M129/12)+(M130/12)+(M131/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C132-C133","v":0},{"$f":"D132-D133","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C134*12","v":0},{"$f":"D134*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","West Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C139-(C140/12)+(C141/12)+(C142/12)","v":0},{"$f":"D139-(D140/12)+(D141/12)+(D142/12)","v":0},{"$f":"E139-(E140/12)+(E141/12)+(E142/12)","v":0},{"$f":"F139-(F140/12)+(F141/12)+(F142/12)","v":0},{"$f":"G139-(G140/12)+(G141/12)+(G142/12)","v":0},{"$f":"H139-(H140/12)+(H141/12)+(H142/12)","v":0},{"$f":"I139-(I140/12)+(I141/12)+(I142/12)","v":0},{"$f":"J139-(J140/12)+(J141/12)+(J142/12)","v":0},{"$f":"K139-(K140/12)+(K141/12)+(K142/12)","v":0},{"$f":"L139-(L140/12)+(L141/12)+(L142/12)","v":0},{"$f":"M139-(M140/12)+(M141/12)+(M142/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C143-C144","v":0},{"$f":"D143-D144","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C145*12","v":0},{"$f":"D145*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Span 4"]
["Slab Location:","East Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C151-(C152/12)+(C153/12)+(C154/12)","v":0},{"$f":"D151-(D152/12)+(D153/12)+(D154/12)","v":0},{"$f":"E151-(E152/12)+(E153/12)+(E154/12)","v":0},{"$f":"F151-(F152/12)+(F153/12)+(F154/12)","v":0},{"$f":"G151-(G152/12)+(G153/12)+(G154/12)","v":0},{"$f":"H151-(H152/12)+(H153/12)+(H154/12)","v":0},{"$f":"I151-(I152/12)+(I153/12)+(I154/12)","v":0},{"$f":"J151-(J152/12)+(J153/12)+(J154/12)","v":0},{"$f":"K151-(K152/12)+(K153/12)+(K154/12)","v":0},{"$f":"L151-(L152/12)+(L153/12)+(L154/12)","v":0},{"$f":"M151-(M152/12)+(M153/12)+(M154/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C155-C156","v":0},{"$f":"D155-D156","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C157*12","v":0},{"$f":"D157*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Reference Line"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C162-(C163/12)+(C164/12)+(C165/12)","v":0},{"$f":"D162-(D163/12)+(D164/12)+(D165/12)","v":0},{"$f":"E162-(E163/12)+(E164/12)+(E165/12)","v":0},{"$f":"F162-(F163/12)+(F164/12)+(F165/12)","v":0},{"$f":"G162-(G163/12)+(G164/12)+(G165/12)","v":0},{"$f":"H162-(H163/12)+(H164/12)+(H165/12)","v":0},{"$f":"I162-(I163/12)+(I164/12)+(I165/12)","v":0},{"$f":"J162-(J163/12)+(J164/12)+(J165/12)","v":0},{"$f":"K162-(K163/12)+(K164/12)+(K165/12)","v":0},{"$f":"L162-(L163/12)+(L164/12)+(L165/12)","v":0},{"$f":"M162-(M163/12)+(M164/12)+(M165/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C166-C167","v":0},{"$f":"D166-D167","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C168*12","v":0},{"$f":"D168*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Crown"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C173-(C174/12)+(C175/12)+(C176/12)","v":0},{"$f":"D173-(D174/12)+(D175/12)+(D176/12)","v":0},{"$f":"E173-(E174/12)+(E175/12)+(E176/12)","v":0},{"$f":"F173-(F174/12)+(F175/12)+(F176/12)","v":0},{"$f":"G173-(G174/12)+(G175/12)+(G176/12)","v":0},{"$f":"H173-(H174/12)+(H175/12)+(H176/12)","v":0},{"$f":"I173-(I174/12)+(I175/12)+(I176/12)","v":0},{"$f":"J173-(J174/12)+(J175/12)+(J176/12)","v":0},{"$f":"K173-(K174/12)+(K175/12)+(K176/12)","v":0},{"$f":"L173-(L174/12)+(L175/12)+(L176/12)","v":0},{"$f":"M173-(M174/12)+(M175/12)+(M176/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C177-C178","v":0},{"$f":"D177-D178","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C179*12","v":0},{"$f":"D179*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","West Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C184-(C185/12)+(C186/12)+(C187/12)","v":0},{"$f":"D184-(D185/12)+(D186/12)+(D187/12)","v":0},{"$f":"E184-(E185/12)+(E186/12)+(E187/12)","v":0},{"$f":"F184-(F185/12)+(F186/12)+(F187/12)","v":0},{"$f":"G184-(G185/12)+(G186/12)+(G187/12)","v":0},{"$f":"H184-(H185/12)+(H186/12)+(H187/12)","v":0},{"$f":"I184-(I185/12)+(I186/12)+(I187/12)","v":0},{"$f":"J184-(J185/12)+(J186/12)+(J187/12)","v":0},{"$f":"K184-(K185/12)+(K186/12)+(K187/12)","v":0},{"$f":"L184-(L185/12)+(L186/12)+(L187/12)","v":0},{"$f":"M184-(M185/12)+(M186/12)+(M187/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C188-C189","v":0},{"$f":"D188-D189","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C190*12","v":0},{"$f":"D190*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Span 5"]
["Slab Location:","East Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C196-(C197/12)+(C198/12)+(C199/12)","v":0},{"$f":"D196-(D197/12)+(D198/12)+(D199/12)","v":0},{"$f":"E196-(E197/12)+(E198/12)+(E199/12)","v":0},{"$f":"F196-(F197/12)+(F198/12)+(F199/12)","v":0},{"$f":"G196-(G197/12)+(G198/12)+(G199/12)","v":0},{"$f":"H196-(H197/12)+(H198/12)+(H199/12)","v":0},{"$f":"I196-(I197/12)+(I198/12)+(I199/12)","v":0},{"$f":"J196-(J197/12)+(J198/12)+(J199/12)","v":0},{"$f":"K196-(K197/12)+(K198/12)+(K199/12)","v":0},{"$f":"L196-(L197/12)+(L198/12)+(L199/12)","v":0},{"$f":"M196-(M197/12)+(M198/12)+(M199/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C200-C201","v":0},{"$f":"D200-D201","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C202*12","v":0},{"$f":"D202*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Reference Line"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C207-(C208/12)+(C209/12)+(C210/12)","v":0},{"$f":"D207-(D208/12)+(D209/12)+(D210/12)","v":0},{"$f":"E207-(E208/12)+(E209/12)+(E210/12)","v":0},{"$f":"F207-(F208/12)+(F209/12)+(F210/12)","v":0},{"$f":"G207-(G208/12)+(G209/12)+(G210/12)","v":0},{"$f":"H207-(H208/12)+(H209/12)+(H210/12)","v":0},{"$f":"I207-(I208/12)+(I209/12)+(I210/12)","v":0},{"$f":"J207-(J208/12)+(J209/12)+(J210/12)","v":0},{"$f":"K207-(K208/12)+(K209/12)+(K210/12)","v":0},{"$f":"L207-(L208/12)+(L209/12)+(L210/12)","v":0},{"$f":"M207-(M208/12)+(M209/12)+(M210/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C211-C212","v":0},{"$f":"D211-D212","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C213*12","v":0},{"$f":"D213*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","Crown"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C218-(C219/12)+(C220/12)+(C221/12)","v":0},{"$f":"D218-(D219/12)+(D220/12)+(D221/12)","v":0},{"$f":"E218-(E219/12)+(E220/12)+(E221/12)","v":0},{"$f":"F218-(F219/12)+(F220/12)+(F221/12)","v":0},{"$f":"G218-(G219/12)+(G220/12)+(G221/12)","v":0},{"$f":"H218-(H219/12)+(H220/12)+(H221/12)","v":0},{"$f":"I218-(I219/12)+(I220/12)+(I221/12)","v":0},{"$f":"J218-(J219/12)+(J220/12)+(J221/12)","v":0},{"$f":"K218-(K219/12)+(K220/12)+(K221/12)","v":0},{"$f":"L218-(L219/12)+(L220/12)+(L221/12)","v":0},{"$f":"M218-(M219/12)+(M220/12)+(M221/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C222-C223","v":0},{"$f":"D222-D223","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C224*12","v":0},{"$f":"D224*12","v":0},0,0,0,0,0,0,0,0,0]
[]
["Slab Location:","West Edge of Deck"]
[null,null,"0/10","1/10","2/10","3/10","4/10","5/10","6/10","7/10","8/10","9/10","10/10"]
["Top of Slab Elev (ft)"]
["- Slab Thickness (in)"]
["+ Camber (in)"]
["+ Falsework Settlement/Deflection (in)"]
["= Top of Falsework Elevation",null,{"$f":"C229-(C230/12)+(C231/12)+(C232/12)","v":0},{"$f":"D229-(D230/12)+(D231/12)+(D232/12)","v":0},{"$f":"E229-(E230/12)+(E231/12)+(E232/12)","v":0},{"$f":"F229-(F230/12)+(F231/12)+(F232/12)","v":0},{"$f":"G229-(G230/12)+(G231/12)+(G232/12)","v":0},{"$f":"H229-(H230/12)+(H231/12)+(H232/12)","v":0},{"$f":"I229-(I230/12)+(I231/12)+(I232/12)","v":0},{"$f":"J229-(J230/12)+(J231/12)+(J232/12)","v":0},{"$f":"K229-(K230/12)+(K231/12)+(K232/12)","v":0},{"$f":"L229-(L230/12)+(L231/12)+(L232/12)","v":0},{"$f":"M229-(M230/12)+(M231/12)+(M232/12)","v":0}]
["- Field Surveyed Top of Installed Falsework Elevation"]
["= 'T' Values (ft)",null,{"$f":"C233-C234","v":0},{"$f":"D233-D234","v":0},0,0,0,0,0,0,0,0,0]
["= 'T' Values (in)",null,{"$f":"C235*12","v":0},{"$f":"D235*12","v":0},0,0,0,0,0,0,0,0,0]

{"sheet":"Locations","index":4,"n_rows":7,"n_cols":1,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["Slab Edge Locations"]
["North Edge of Deck"]
["East Edge of Deck"]
["South Edge of Deck"]
["West Edge of Deck"]
["Reference Line"]
["Crown"]