Click here to enter a date.

## Project info

|  |  |  |  |
| --- | --- | --- | --- |
| Project ID  |       | Structure ID(s)  |       |
| Contract ID  |       |  |       |
| Highway  |       |  |       |
| Description  |       |  |       |
| County  |       |  |       |

## Introductions / pour day contacts

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | **Name** | **Phone** | **Attended Meeting** |
| Project Leader |  |       |       | **[ ]**  |
| Lead Inspector |  |       |       | **[ ]**  |
| Contractor |  |       |       | **[ ]**  |
| QC Testing |  |       |       | **[ ]**  |
| Concrete Supplier |  |       |       | **[ ]**  |
| WisDOT Materials |  |       |       | **[ ]**  |
| Contractor Materials |  |       |       | **[ ]**  |
| Independent Assurance |  |       |       | **[ ]**  |
| Additional Meeting Attendees |  |       |       |  |
|  |       |       |  |
|  |       |       |  |

## QMP Plan

|  |  |
| --- | --- |
| Submitted | Click here to enter a date. |
| Reviewed  | Click here to enter a date. |
| Accepted  | Click here to enter a date. |
| Accepted QMP Plan Distributed to | [ ]  QC Tester |
|  | [ ]  QV Tester |

## Concrete Mixtures

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  | **Special Considerations** | **Yes** | **No** |
| Plant/Back up Location |       |  | Seal pour | **[ ]**  | **[ ]**  |
| Mix IDs/type |       |  | HPC | **[ ]**  | **[ ]**  |
| Number of trucks /rate of delivery |       |  | Modified HPC | **[ ]**  | **[ ]**  |
| WS5014 Signed for all mix designs | Click here to enter a date. |  | Other (list) | **[ ]**  | **[ ]**  |
| **REMINDER: Batch tickets required with each load. (SS 501.3.5.4(2))** |  |

## Construction Schedule

|  |  |
| --- | --- |
| Anticipated pour date | Click here to enter a date. |
| Back up date | Click here to enter a date. |
| Estimated pour start |       |
| Dry run date /check fogging equipment | Click here to enter a date. |
|  |  |

## Temperature Control Plan

### Hot Weather concreting (ss 501.3.8.2)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Temp Control Plan** | **Actions to Control Concrete Temperature** | **Yes** | **No** | **Remarks** |
| Submitted | Click here to enter a date. |  | Cool Aggregate | **[ ]**  | **[ ]**  |       |
| Accepted  | Click here to enter a date. |  | Cold Batch Water | **[ ]**  | **[ ]**  |       |
|  |  |  | Pour Time | **[ ]**  | **[ ]**  |       |
|  |  |  | Others (list) | **[ ]**  | **[ ]**  |       |

*If* ***ICE*** *is to be added,* ***ALL OTHER METHODS MUST BE USED FIRST.***

|  |  |
| --- | --- |
| Timeframe for Ordering and Adding Ice |       |
| Ice Compensation Expectations [Per Section 501.3.8.2.1(1)] |       |
|  |  |
| EVAPORATION PLAN ( SS 501.3.8.2.2) |  |
| Date Submitted Click here to enter a date. |  |
| Date Accepted Click here to enter a date. |  |

### Cold Weather Protection (SS 502.3.9)

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Yes** | **No** | **Remarks** |
| Heat Forms | [ ]  | [ ]  |       |
| Heat Batch Water | [ ]  | [ ]  |       |
| Heat Aggregate | [ ]  | [ ]  |       |
| Temp Probe Frequency | [ ]  | [ ]  |       |
| Others (list) | [ ]  | [ ]  |       |

## Curing Process

|  |  |
| --- | --- |
|  Normal deck wet cure 7 days (502.3.8.2.3) |       |
| HPC wet cure for 14 days (see special provisions) |       |
| Deck overlay wet cure 3 days (509.3.9.3) |       |
| Strength Verification (502.3.10) | [ ]  Maturity | [ ]  Cylinders | [ ]  Time  | [ ]  Other (list) |

## Placement

|  |  |  |
| --- | --- | --- |
| Truck Access |  |       |
|  Placement Method |  | [ ]  Bucket | [ ]  Pump | [ ]  Bucket & Pump | [ ]  Mobile Mix [ ]  Other (list) |
| If pump, air loss <1%  |  | (502.3.5.1(11)) |  |  |  |
| Truck Washout |  |       |
| Type of consolidation |  |       |
| # of people on pour |  |       |
| Fogging |  |       |
| Back-up equipment |  |       |
| Additional Traffic control  |  |       |

## Sampling and testing

|  |  |  |
| --- | --- | --- |
| Testing Location  |       |  |
| Cylinder Storage Location |       |  |
| Tester Access  |       |  |
| QC Sublot/lot received? |       |  |
| QC aggregate testing (plant or contract)? |       |  |

**REMINDER: Sampling must be at the** **point of placement and between 10% and 90% of the load.**

### Communication reminders

|  |  |
| --- | --- |
| **Test results** |  |
| Delivery method |       |
| Frequency |       |

* + Random Numbers computed on amount placed
	+ QC Plan actions to be followed for failing tests
	+ ***QV & QC are required to inform each other of failing results immediately***
	+ Nonconforming material to be discarded
	+ Nonconforming material left in place to be quantified and agreed to with the engineer
	+ Changes in mix designs/sources must be communicated and approved before they happen. Testing may have to be adjusted to accommodate the change. Contractor must inform all parties of the change.
	+ **Final Report – 10 days after last 28-day breaks is completed. Organization expectations?**
	+ **QC & QV check in after pour is completed**

## Inspection Reminders

* + Surveyed by contractor and checked separately by inspectors
	+ Deck Overlays max air temp of 88 degrees F (509.3.9.2)
	+ Engineer must give written permission to proceed with pour (501.3.8.2.2(5))
	+ Where can emergency header be placed?
	+ Finishing texture (502.3.7.8)
	+ Emergency cover material?
	+ Bar steel checked for size, spacing, tying, clearances, and cleanliness
	+ Forms checked and found clean, oiled, and locked
	+ Bracing checked & secured

|  |  |
| --- | --- |
| * + 24-hr contact for curing issues
 |  |
| Name |       |
| Phone |       |

## Other Issues or Concerns

|  |
| --- |
| STANDARD SPEC REQUIREMENTS |

* Slump: 1”-4” (501.3.7.1), deck overlay grade E, see 509.2
* Air: 6% +/-1.5% (501.3.2.4.2), grade E 6% +/- 1.0%
* Discharge time: 501.3.5.2
* Review Special Provisions for exceptions to standard requirements