NUCLEAR SOILS DENSITY TESTING RECORDS	Wisconsin Department of Transportation
WS4601
Project ID:	Road Name:	Project Engineer:
Contractor:	County:	Region:	Hwy. No.:
Operator:	Set No.	Density Standard	Moisture Standard	Date:
Test No.
Grading Area
Station
Offset
Depth Below Subgrade
Test Position B.S. or D.T. Depth ,4",6"or 8"
Required % of Maxium Density
Contact Reading
Density Count
Air Gap Reading
Wet Density (P.C.F.)
Total Density
Moisture Count
Moisture (P.C.F.) (b)
Total Water
Bulk Dry (c)
Dry Density
% Moisture 100 x b / c
% Maximum Density 100 x c / d
Soils Classification
Proctor Number Pit Number
Maximum Density (d) of Proctor
Proctor Optium Moisture
% R-4 Material
Test Remarks